Configuração do Switch

|  |
| --- |
| configure terminal  interface fastethernet 0/1  switchport mode access  switchport access vlan y0  exit  interface fastethernet 0/5  switchport mode access  switchport access vlan y0  exit  interface fastethernet 0/3  switchport mode access  switchport access vlan y1  exit  interface fastethernet 0/7  switchport mode access  switchport access vlan y1  exit  interface fastethernet 0/9  switchport mode access  switchport access vlan y1  exit  interface fastethernet 0/11  switchport mode access  switchport access vlan 1  end  show vlan brief |

Configuração do Router

|  |
| --- |
| configure terminal  access-list 1 permit 172.16.50.0 0.0.0.255  access-list 1 permit 172.16.51.0 0.0.0.255  interface gigabitethernet 0/0  ip address 172.16.51.254 255.255.255.0  no shutdown  ip nat inside  exit  interface gigabitethernet 0/1  ip address 172.16.1.59 255.255.255.0  no shutdown  ip nat outside  exit  ip route 0.0.0.0 0.0.0.0 172.16.1.254  ip route 172.16.50.0 255.255.255.0 172.16.51.253  ip nat pool ovrld 172.16.1.59 172.16.1.59 prefix 24  ip nat inside source list 1 pool ovrld overload  end  show interface gigabitethernet 0/0  show interface gigabitethernet 0/1  show ip route |



